### Connection Accessories

uPyxis Desktop needs some accessories to connect to Pyxis devices

To connect to a Bluetooth enabled device, a USB-Bluetooth adapter (Part Number: MA-NEB) is needed.
To connect to a WiFi enabled device, please make sure the PC has a WiFi connection. Almost all laptop computers have WiFi nowadays, but some desktop computers don't have WiFi adapters.

### Supported Devices

uPyxis Desktop will keep adding more supported devices. The following list shows the supported devices by the current version.

Inline Devices

- ST-601 ClO2 Sensor
- CR-300 / CR-200 Corrosion Rate Sensor
- LS-202 Ultrasonic Level Sensor

To connect to an inline device, a USB adapter (Part Number: MA-WB) is needed to connect to the inline device. Please refer to the device instruction manual for more information at http://www.pyxis-lab.com/support.html.

Looking for something not on the list? Please send an email to service@pyxis-lab.com.

### Mobile Apps

uPyxis also has its mobile apps for iOS and Android. The apps can set the device, do a calibration, and upload diagnosis data for inline devices. It also can change the setting of handheld devices and export device data log.

Please search "uPyxis" on the Apple App Store or Google Play Store, or click the links below for more information

### More Information

If your Pyxis meter or probe requires service please send an email to service@pyxis-lab.com.